Specification

• CCD: Hamamatsu S5466

type 2 phase FFT-CCD number of pixels 512×512 pixel size 24μm×24μm sensitive area 12.3mm×12.3mm active layer in depth ∼10μm^† sensitivity 2.0μV/e^− charge transfer eff. >0.99995 †50μm type (special made) is also used in the exp.

• Driver: Hamamatsu C5934-1010^‡

gain ×55 H-clock 250kHz V-clock 62.5kHz noise w/CCD 20e^− operation mode normal/MPP ‡C5934-0909 (low gain) is also used in the exp.