MPP (Multi Pinned Phase) Operation

“Inverted Operation” in other words

• Holes are accumulated under S_i/S_iO_2 interface. • Thermal excitation of e^− is significantly suppressed.

⇒ Reduction of the dark current by factor 10

MPP mode

• 2 phase CCD: potential wells even when P 1V = P 2V

HPK S5466/C5934 achieves MPP operation