Experimental condition

• Temperature: −15^∘C, −5^∘C, +5^∘C, +15^∘C • Incidence: 0^∘, 45^∘, 60^∘ • Readout cycle: 4sec, 1.3sec

Beam off data ⇒ Properties of dark current Beam on data ⇒ MIP measurement