Gain & Readout noise

The analysis of σnoise vs dark current gives

CCD1 CCD2 CCD3 Gain(μV/e^−) 103.2±2.3 10.6±1.4 99.7±2.1 R/O Noise(mV) 1.6±0.4 0.5±0.3 1.7±0.3

Readout noise for ready-made CCD’s is consistent with the specification: 20e^− ⇒ 2.0mV

Direct calibration using^{109}Cd (X-rays: 22keV, 26keV)

CCD1 CCD2 CCD3 Gain(μV/e^−) 100.2±0.1 9.6±0.1 112.6±0.1